**711-1100 Cast Aluminum Pole Vault Box**

SECTION 11 68 33.43 Track and Field Equipment

**PART 1 GENERAL**

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 711-1100 Cast Aluminum Pole Vault Box

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Section 02200 – Earthwork; Excavation and Backfill and

establishment of sub-grade elevations.

2. Section 02511 – Asphalt, Concrete, and Pavement

3. Section 02535 – Synthetic Track Surfacing

4. Section 02542 – Synthetic Field Surfacing

5. Section 03300 – Cast-in-Place Concrete

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF) 2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, not including powder coating.

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 CAST Aluminum Pole Vault Box with Cover**

**A**. 711-1100 Cast Aluminum Pole Vault Box having the following attributes:

A. Regulation Size

B. Cast Aluminum Setting Wings for Concrete Encasement

C. Powder Coating White (Yellow Available)

D. **WORLD ATHLETICS CERTIFICATE:** E-99-0061

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**

**711-1200 Stainless Steel Pole Vault Box**

SECTION 11 68 33.43 Track and Field Equipment

**PART 1 GENERAL**

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 711-1200 Stainless Steel Pole Vault Box

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Section 02200 – Earthwork; Excavation and Backfill and

establishment of sub-grade elevations.

2. Section 02511 – Asphalt, Concrete, and Pavement

3. Section 02535 – Synthetic Track Surfacing

4. Section 02542 – Synthetic Field Surfacing

5. Section 03300 – Cast-in-Place Concrete

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF) 2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Stainless Steel Pole Vault Box**

**A.** 711-1200 Pole Vault Box fabricated with 12 gage stainless steel having the following attributes:

A. Regulation Size

B. Stainless Steel Setting Wings for Concrete Encasement

C. Powder Coating White (Yellow Available)

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**

**711-1400 Vault Box Cover- Recessed**

SECTION 11 68 33.43 Track and Field Equipment

PART 1 GENERAL

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 711-1400 Galvanized Steel Vault Box Cover- Depressed

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Section 02200 – Earthwork; Excavation and Backfill and

establishment of sub-grade elevations.

2. Section 02511 – Asphalt, Concrete, and Pavement

3. Section 02535 – Synthetic Track Surfacing

4. Section 02542 – Synthetic Field Surfacing

5. Section 03300 – Cast-in-Place Concrete

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF) 2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Vault Box Cover- Depressed**

**A.** 711-1400 Vault Box Cover fabricated with 0.25” Galvanized Steel having the following attributes:

A. Sized to Fill Void of Standard Vault Box

B. Top Surface Recessed 0.50in to Accept Synthetic Track Material

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**

**711-1401 Vault Box Cover- Flush**

SECTION 11 68 33.43 Track and Field Equipment

PART 1 GENERAL

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 711-1401 Vault Box Cover**-** Flush

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Section 02200 – Earthwork; Excavation and Backfill and

establishment of sub-grade elevations.

2. Section 02511 – Asphalt, Concrete, and Pavement

3. Section 02535 – Synthetic Track Surfacing

4. Section 02542 – Synthetic Field Surfacing

5. Section 03300 – Cast-in-Place Concrete

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF) 2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Vault Box Cover- Flush**

**A**. 711-1401 Vault Box Cover fabricated with 0.25” Galvanized Steel having the following attributes:

1. Sized to Fill Void of Standard Vault Box

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**