**712-1150 Communication Box for Synthetic Turf**

SECTION 11 68 33 Athletic Field Equipment

**PART 1 GENERAL**

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 712-1150 Communication Box for Synthetic Turf

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Division 03 – Concrete; Sections: Cast-in-Place Concrete
2. Division 26 – Electrical
3. Division 27 – Communications
4. Division 31 – Earthwork; Sections: Excavation and Backfill and Establishment of Sub-Grade Elevations
5. Division 32 – Exterior Improvements; Sections: Athletic and Recreational Surfacing, Concrete and Asphalt
6. Division 33 – Utilities

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF)

2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Communication box for synthetic turf**

**A**. 712-1150 Communication Box for Synthetic Turf

Box:¼” Aluminum, TIG Welded with open bottom

Lid:Break formed ¼” Aluminum

Recessed Cover for synthetic surfacing (To be applied by Surfacing Contractor)

Overall size 36.38”Lx19.25” Wx12.81”D

Optional- Divider welded or removable as per customer’s request

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**

**712-1160 Communication Box with Mat Filler Kit**

SECTION 11 68 33 Athletic Field Equipment

**PART 1 GENERAL**

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 712-1160 Communication Box with Mat Filler Kit

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Division 03 – Concrete; Sections: Cast-in-Place Concrete
2. Division 26 – Electrical
3. Division 27 – Communications
4. Division 31 – Earthwork; Sections: Excavation and Backfill and Establishment of Sub-Grade Elevations
5. Division 32 – Exterior Improvements; Sections: Athletic and Recreational Surfacing, Concrete and Asphalt
6. Division 33 – Utilities

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF)

2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Communication box with mat filler Kit**

**A**. 712-1160 Communication Box with Mat Filler Kit

Box:¼” Aluminum, TIG Welded with open bottom

Lid:Break formed ¼” Aluminum

Recessed Cover for Mat Filler Kit

Overall size 36.38”L x 19.25”W x 12.81”D

Optional- Divider welded or removable as per customer’s request

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**

**712-1250 Communication Box for Artificial Turf**

SECTION 11 68 33 Athletic Field Equipment

**PART 1 GENERAL**

**1.1 WORK INCLUDED**

**A.** Provide all equipment and materials, and do all work necessary to furnish

and install the athletic equipment, as indicated on the drawings and as

specified herein. Athletic equipment shall include, but not be limited to:

1. 712-1250 Communication Box for Artificial Turf

**1.2 RELATED WORK**

**A.** Examine contract documents for requirements that affect work of this

section. Other specification sections that directly relate to the work of

this section include, but are not limited to:

1. Division 03 – Concrete; Sections: Cast-in-Place Concrete
2. Division 26 – Electrical
3. Division 27 – Communications
4. Division 31 – Earthwork; Sections: Excavation and Backfill and Establishment of Sub-Grade Elevations
5. Division 32 – Exterior Improvements; Sections: Athletic and Recreational Surfacing, Concrete and Asphalt
6. Division 33 – Utilities

**1.3 REFERENCES**

**A.** Comply with applicable requirements of the following standards. Where

these standards conflict with other specified requirements, the most

restrictive requirements shall govern.

1. World Athletics (Formerly IAAF)

2. National Collegiate Athletic Association (NCAA)

3. National Federation of State High School Associations (NFHS)

4. American Sports Builders Association (ASBA)

5. Manufacturers Data and Recommended Installation

Requirements

**1.4 SUBMITTALS**

**A.** Manufacturers Product Data

1. Provide manufacturers product data prior to actual field

installation work, for Architects or Owners representatives

review.

**B.** Shop Drawings

1. Provide drawings of the manufacturers recommended

installation and foundation requirements prior to actual field

installation work, for Architects or Owners representatives

review.

**1.5 QUALITY ASSURANCE**

**A.** Manufacturers warranties shall pass to the Owner and certification made

that the product materials meet all applicable grade trademarks or conform to industry standards and inspection requirements.

**B.** Single Source Responsibility: Provide equipment from single manufacturer

**C.** Manufacturer’s Qualifications: Minimum of 7 consecutive years experience manufacturing items similar to that specified.

**1.6 PRODUCT DELIVERY AND STORAGE**

**A.** Materials delivered to the site shall be examined for damage or defects in shipping. Any defects shall be noted and reported to the Owners representative. Replacements, if necessary, shall be immediately re- ordered, so as to minimize any conflict with the construction schedule. Sound materials shall be stored above ground under protective cover or indoors so as to provide proper protection.

**1.7 WARRANTY**

**A.** Provide 3-year warranty against defects in materials and workmanship, unless otherwise specified

**PART 2 PRODUCTS**

**2. 1 MANUFACTURERS**

**A.** Acceptable Manufacturer: UCS, Inc. 511 Hoffman Road, Lincolnton, NC 28092, phone 800-526-4856, fax 704-732-9559, web address: www.ucsspirit.com

**B.** Substitutions:Not Permitted

**2.2 Communication box for artificial turf**

**A**. 712-1250 Communication Box for Artificial Turf

Box:¼” Aluminum, TIG Welded with open bottom

Lid:Break formed ¼” Aluminum

Includes ¼” Aluminum plate with pressure treated plywood cover to apply turf to (Supplied by Contractor).

Overall size 36.38”L x 19.25”W x 12.81”D

Optional- Divider welded or removable as per customer’s request

# **PART 3 EXECUTION**

**3.1 INSTALLATION OF EQUIPMENT**

**A.** All athletic equipment shall be installed as recommended with manufacturer's written directions, and as indicated on the drawings.

**END OF SECTION**